STRUCTURE Safe and sound, quality controlled RCC frame structure with best material components Earthquake resistant design.

PLASTER WORK Double coat plaster on external walls, single coat plaster in inside area flooring and wall.

TILING Vitrified tiles size 2'x2' flooring having greater strength in entire area.

ELECTRICAL WORK 3 phase concealed and fire resistant right gauge wiring of ISI copper wire Distribution board with MCB ISI mark modular electrical accessories.

PAINTING Long lasting and weather resistant acrylic paint of standard make to all external walls All internal walls with white cement based putty finish with OBD.

PLUMBING AND SANITATION Good quality designer sanitary ware for spotless and sparkling toilets High quality plumbing fixtures Corrosion free and leak proof CPVC/UPVC pipe and fitting(ISI make) SWR drainage system for easy maintenance.

LOBBY AND STAIRCASE All lobby, staircase and corridors in soothing Granite stone with S.S. railing.